{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["TNB Statikkonsole"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TNB Statikkonsole","index":0,"n_rows":43,"n_cols":53,"rows_kept":43,"cut":false,"hidden":false,"merged":[[9,2,9,16],[5,0,5,1],[7,0,7,1],[5,7,5,10],[7,7,7,10],[7,15,7,16],[7,11,7,14],[5,2,5,5],[7,2,7,5],[5,11,5,16]]}
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Alternative:"]
["Prüfklasse",null,"B",null,null,null,null,"Kastengrösse",null,null,null,"TNB 260x275 RI/RA/RS",null,null,null,null,null,null,null,null,null,"> 10 Konsolen",null,null,null,null,null,null,null,null,"Berechnung mit Tastenkombination [strg]+[s] starten."]
[]
["Windklasse",null,3,null,null,null,null,"Trägheitsmoment",null,null,null,2.4000000953674316,null,null,null,"cm^4"]
[]
["Statikeisen",null,"Statikeisen Hebe-Schiebe-Türe"]
[]
["Breite cm",90,100,110,120,130,140,150,160,170,180,190,200,210,220,230,240,250,260,270,280,290,300,310,320,330,340,350,360,370,380,390,400,410,420,430,440,450,460,470,480,490,500,510,520,530,540,550,560,570,580,590,600]
["Höhe cm"]
[90,"-","-","-","-","-","-","-","-","-","SP","SP","SP","SP","SP",1,1,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,3,3,3,3,3]
[100,"-","-","-","-","-","-","-","-","SP","SP","SP","SP","SP",1,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,3,3,3,3,3,3,3,3,4,4]
[110,"-","-","-","-","-","-","-","-","SP","SP","SP","SP",2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4]
[120,"-","-","-","-","-","-","-","SP","SP","SP","SP",2,2,2,2,2,2,2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,4,4,4,4,4]
[130,"-","-","-","-","-","-","-","SP","SP","SP","SP",2,2,2,2,2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,4,4,4,4,4,5,5,5]
[140,"-","-","-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,4,4,4,4,5,5,5,5,5,5,5]
[150,"-","-","-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,4,4,4,5,5,5,5,5,5,5,5,5,5,5]
[160,"-","-","-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,4,4,5,5,5,5,5,5,5,5,5,5,6,6,6,6]
[170,"-","-","-","-","-","-","SP","SP","SP","SP",2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,4,5,5,5,5,5,5,5,5,5,6,6,6,6,6,6,6]
[180,"-","-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,4,5,5,5,5,5,5,5,5,5,6,6,6,6,6,6,6,6,6]
[190,"-","-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,2,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,5,5,5,5,5,5,5,5,5,6,6,6,6,6,6,6,6,7,7,7]
[200,"-","-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,2,3,3,3,3,3,3,3,4,4,4,4,4,4,4,4,5,5,5,5,5,5,5,5,6,6,6,6,6,6,6,6,7,7,7,7,7]
[210,"-","-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,3,3,3,3,3,3,3,3,4,4,4,4,4,4,4,5,5,5,5,5,5,5,6,6,6,6,6,6,6,7,7,7,7,7,7,7,7]
[220,"-","-","-","-","-","SP","SP","SP","SP",2,2,2,2,2,2,3,3,3,3,3,3,3,4,4,4,4,4,4,4,5,5,5,5,5,5,5,6,6,6,6,6,6,6,7,7,7,7,7,7,7,8,8]
[230,"-","-","-","-","-","SP","SP","SP","SP",2,2,2,2,2,2,3,3,3,3,3,3,4,4,4,4,4,4,4,5,5,5,5,5,5,5,6,6,6,6,6,6,7,7,7,7,7,7,7,8,8,8,8]
[240,"-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,2,3,3,3,3,3,3,4,4,4,4,4,4,5,5,5,5,5,5,6,6,6,6,6,6,6,7,7,7,7,7,7,8,8,8,8,8,8]
[250,"-","-","-","-","-","SP","SP","SP",2,2,2,2,2,2,2,3,3,3,3,3,3,4,4,4,4,4,4,5,5,5,5,5,5,6,6,6,6,6,6,7,7,7,7,7,7,8,8,8,8,8,8,9]
[260,"-","-","-","-","SP","SP","SP","SP",2,2,2,2,2,2,2,3,3,3,3,3,4,4,4,4,4,4,5,5,5,5,5,5,6,6,6,6,6,6,7,7,7,7,7,8,8,8,8,8,8,9,9,9]
[270,"-","-","-","-","SP","SP","SP","SP",2,2,2,2,2,2,2,3,3,3,3,3,4,4,4,4,4,4,5,5,5,5,5,6,6,6,6,6,6,7,7,7,7,7,8,8,8,8,8,8,9,9,9,9]
[280,"-","-","-","-","SP","SP","SP",1,2,2,2,2,2,2,2,3,3,3,3,3,4,4,4,4,4,5,5,5,5,5,5,6,6,6,6,6,7,7,7,7,7,8,8,8,8,8,9,9,9,9,9,9]
[290,"-","-","-","-","SP","SP","SP",1,2,2,2,2,2,2,2,3,3,3,3,3,4,4,4,4,4,5,5,5,5,5,6,6,6,6,6,7,7,7,7,7,8,8,8,8,8,9,9,9,9,9,10,10]
[300,"-","-","-","-","SP","SP","SP",1,2,2,2,2,2,2,2,3,3,3,3,3,4,4,4,4,4,5,5,5,5,5,6,6,6,6,7,7,7,7,7,8,8,8,8,8,9,9,9,9,9,10,10,10]
[310,"-","-","-","-","SP","SP","SP",1,2,2,2,2,2,2,2,3,3,3,3,3,4,4,4,4,4,5,5,5,5,6,6,6,6,6,7,7,7,7,7,8,8,8,8,9,9,9,9,9,10,10,10,10]
[320,"-","-","-","SP","SP","SP","SP",1,2,2,2,2,2,2,2,3,3,3,3,3,4,4,4,4,5,5,5,5,5,6,6,6,6,7,7,7,7,7,8,8,8,8,8,9,9,9,9,10,10,10,10,10]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Version: 3.00"]
["Legende:",null,null,null,null,null,null,null,"Folgende Voraussetzungen sind zu beachten:"]
["SP = Statikprofil",null,null,null,null,null,null,null,"1.) Systemvorgaben der Fenster- und Glashersteller sind zu beachten."]
["Zahl = Anzahl Verstärkungskonsolen",null,null,null,null,null,null,null,"2.) Geeignete Befestigungsmaterialien je nach Befestigungsgrund sind zu verwenden."]
["Maßtabelle = Elementmaß inkl. Kasten",null,null,null,null,null,null,null,"3.) Angaben beziehen sich ausschließlich auf Windwiederstand (vertikale Kräfte sind nicht berücksichtigt)."]
[null,null,null,null,null,null,null,null,"4.) Die Berechnungen beziehen sich auf die DIN 18055:2014-14 Kriterien für die Anwendung von Fenstern und Außentüren nach DIN EN 14351-1"]